|  |  |  |
| --- | --- | --- |
|  | SAN DIEGO AIR POLLUTION CONTROL DISTRICT**COMPLIANCE DIVISION**10124 Old Grove RoadSAN DIEGO CA 92131PHONE (858) 586-2650 FAX (858) 586-2651 | APCD USE ONLY |
| SECTOR |
| ID# |
| NOV# |

**ISD OPERABILITY TEST PROCEDURE**

##### **Exhibit 9 of ARB E.O. VR 202-XX**

**Facility Name:**       **A/C or PO Number:**       **Time of Test:**

 (Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A )

|  |
| --- |
| **For ISD Alarm Response Purposes only**: ISD Pressure Sensor verified to be in proper orientation: [ ]  Yes or [ ]  No |

|  |  |
| --- | --- |
| **Pressure Sensor Location:**Dispenser No.:       /        | **Pressure Sensor Serial No.**        |
| **Ullage Pressure from Digital Manometer**       **Pressure from TLS Console**     **Compare the two readings and enter the difference**       **”w.c.**  |
| **Non-Calibrated Sensor Value** **“w.c.**  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Dispenser1** | **Fueling Point2** | **Vapor Flow Meter Serial No.3** | **Real Time A/L Values from PC Setup Tool4** | **V/L****reading** **for the lowest grade per Exhibit 5** | **V/L Difference****(Real Time A/L From PC Setup Tool Minus V/L From Test)6** | **Pass/****Fail7** | Additional V/L readings for the lowest grade per Exhibit 5**(If Required)8** | **Average of 3 V/L readings** **(per Exhibit 5)9** | **Pass/****Fail10** |
| **#2** | **#3** |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |

|  |  |  |
| --- | --- | --- |
|  | SAN DIEGO AIR POLLUTION CONTROL DISTRICT**COMPLIANCE DIVISION**10124 Old Grove RoadSAN DIEGO CA 92131PHONE (858) 586-2650 FAX (858) 586-2651 | APCD USE ONLY |
| SECTOR |
| ID# |
| NOV# |

**Exhibit 9 of ARB E.O. VR 202-XX**

**Facility Name:**        **A/C or PO Number:**       **Time of Test:**

 (Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Dispenser1** | **Fueling Point2** | **Vapor Flow Meter Serial No.3** | **Real Time A/L Values from PC Setup Tool4** | **V/L****reading** **for the lowest grade per Exhibit 5** | **V/L Difference****(Real Time A/L From PC Setup Tool Minus V/L From Test)6** | **Pass/****Fail7** | Additional V/L readings for the lowest grade per Exhibit 5**(If Required)8** | **Average of 3 V/L readings** **(per Exhibit 5)9** | **Pass/****Fail10** |
| **#2** | **#3** |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |
|       |       |       |       |       |       |       |       |       |       |       |

|  |
| --- |
| **Site Shutdown Test**Is the power to submersible pumps off after removing power from TLS Console?[ ] Yes [ ] No*There shall be no dispensing when the TLS power is off**Must be performed by a certified Veeder Root contractor.* |

