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COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131-1649 PHONE (858) 586-2650


VP1000/DISPENSER INTEGRITY TEST
Exhibit 14 & IOM of VR 201/202


Facility Name:	A/C or PO Number:	Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A)


	
Dispenser No.
	Exhibit 14 & IOM B-3
	Exhibit 14 & IOM B-4
	IOM B-5
	IOM B-6

	
	Vacuum Reading Initial1 (WC)
	Vacuum Reading After closing the ball valve1
(WC)
	Vacuum Reading After 60 sec.2 (WC)
	
Dispenser Side
	Dispensing Vacuum3 (WC)
	
Change in Speed (check one)
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	☐ YES  ☐ NO
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1 These vacuum readings shall be at least 60” Water Column (WC)
2 Final vacuum reading shall not fall more than 4” WC from the reading taken after closing the ball valve.
3 The dispensing vacuum shall not be less than 60” WC
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