[image: ]SAN DIEGO AIR POLLUTION CONTROL DISTRICT COMPLIANCE DIVISIONAPCD USE ONLY
SECTOR
ID#
NOV#


10124 OLD GROVE ROAD SAN DIEGO, CA 92131-1649 PHONE (858) 586-2650

Exhibit 15 ARID Technologies AT-150 Permeator Compliance Test Data

	Facility Name:
	
	A/C or PO Number:
	 

	Time of Test:
	
	Starting Pressure:
	



Revision 03/21

(Record exact time of test in order to demonstrate proper test     sequencing as required in Attachment A or L)


Certified Permeator Technician (CPT):

Certification # (as applicable):

ICC or District Training Certification (as applicable):







Calibration Gas Concentration (% Propane). Note: Calibration gas information listed in Section 4 of Exhibit 15 shall be attached to this form.
	Calibration Gas (as applicable):
	Serial #:

	Zero Gas:
	
	

	Low-Range Gas:
	
	

	High-Range Gas:
	
	



NOVA Analyzers:
	Measurement
	Time:
	HC Analyzer Reading
	Average of Measurements
	Maximum
Average HC allowed
	Pass/Fail

	1 (10 mins)
	
	
	
	

≤ 3.0%
	 
	2 (15 mins)
	
	
	
	
	

	3 (20 mins)
	
	
	
	
	

	4 (25 mins)
	
	
	
	
	

	5 (30 mins)
	
	
	
	
	



RKI Analyzers (RKI Eagle2 and RKI GX-6000)
	Measurement
	Time:
	HC
Analyzer Reading
	HC Analyzer Reading (below 100% of LEL)1
	Average of Measurements
	Maximum Average HC allowed
	Pass/Fail

	1 (10 mins)
	
	
	
	
	

≤ 3.0%
	 
	2 (15 mins)
	
	
	
	
	
	

	3 (20 mins)
	
	
	
	
	
	

	4 (25 mins)
	
	
	
	
	
	

	5 (30 mins)
	
	
	
	
	
	



[bookmark: _bookmark0]1: For measured gas concentration below 100% of LEL (Lower Explosive Limit), the values will be % of LEL. Use the equation: % of LEL x 2.1 = % HC as C3 by volume
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