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COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131-1649 PHONE (858) 586-2650

[bookmark: OF_THE_HEALY_CLEAN_AIR_SEPARATOR]DETERMINATION OF STATIC PRESSURE PERFORMANCE OF THE HEALY CLEAN AIR SEPARATOR
Exhibit 4 of ARB E.O. VR-201/202-XX and Exhibit 14 of ARB E.O VR-203/204-XX

	
Facility Name:	A/C or PO Number:		Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A)For ISD Alarm Response Purposes Only: CAS Ball Valve positions checked for proper orientations:	☐ Yes or	☐ No



	Time and Date of most recent delivery: 
	Leak Check Conducted:	☐ Yes or	☐ No

	Date of Last Calibration of Pressure Measurement Device: 
	Phase II Executive Order #: 



If the station pressure is -2.00” W.C. or more negative, a vacuum test must be performed followed by a pressure test. If the pressure is less negative than -2.00” W.C., a pressure test must be performed. Anytime a vacuum test is conducted a subsequent pressure test shall also be conducted immediately after the vacuum test.

Existing station pressure: 		
VACUUM TEST	PRESSURE TEST
	Time (Minutes)
	Vacuum Measurement (in wc)
	
	Time (Minutes)
	Pressure Measurement (in wc)

	Beginning of Test
	
	
	Beginning of Test
	

	At 1 minute
	
	
	At 1 minute
	

	At 2 minutes
	
	
	At 2 minutes
	

	At 3 minutes
	
	
	At 3 minutes
	

	At 4 minutes
	
	
	At 4 minutes
	

	At 5 minutes
	
	
	At 5 minutes
	

	Allowable Minimum Vacuum (from Table 1)
	
	
	Allowable Final Pressure
	1.77
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