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COUNTY OF SAN DIEGO 10124 OLD GROVE ROAD SAN DIEGO CA 92131
PHONE (858) 586-2600


VAPOR RETURN LINE VACUUM INTEGRITY TEST

[bookmark: ARB_EO_G-70-187,_Exhibit_4_,_Healy_400_o]ARB EO G-70-187, EXHIBIT 4 , HEALY 400 ORVR NOZZLES ONLY

Facility Name:		A/C or PO Number:		Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment B)

	Pressure Gauge Calibration Data

Make/Model:		Serial #:		 Calibration date:			
(Calibration should be conducted at a frequency not to exceed 90 days)
	
Equation
1st) Measured DP= The observed change in vacuum level in inches of water column from the initial vacuum from the vacuum after 5 minutes.
2nd) Calculated DP=800/N
Where: N=The approximate length of 2” vapor return pipe from the dispensers to the central vacuum unit to the nearest 20 feet.
3rd) Compare the Measured DP to the Calculated DP (If the Measured DP is greater than the calculated DP then a vapor leak is evident and the system has failed).

	
Length of Vapor Return Line=	
The approximate length of 2 inch vapor return (VR) pipe from the dispensers to the central vacuum unit (CVU) to the nearest 20 feet. Length Determined by:
Blueprints ☐ Inspection ☐ Permit ☐
*If the value is described on the permit no other value can be used.
	

	
	Test Results
	
	

	Diameter of Vapor Return Line:	2” ☐	3” ☐
	Measured DP= 	
	calculated DP=
	

	
	
	
	

	If the site contains 3” vapor return pipes, multiply calculated DP by 0.5.
	Starting Vacuum Level: ”
	
	

	If the system contains more than one Central Vacuum Unit (CVU) with separate piping, repeat test for each CVU and its associated piping.
	1 Minute:	”
2 Minute:	”
	
	

	
	3 Minute:	”
	
	

	
	4 Minute:	”
	
	

	
	Final Vacuum Level@ 5 Minutes:
	”
	

	
	Final Test Results:	Pass ☐
	Fail ☐
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