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[bookmark: Exhibit_8_of_ARB_E.O._VR_203-X_and_VR-20]VST ECS HYDROCARBON SENSOR VERIFICATION TEST PROCEDURE
Exhibit 8 of ARB E.O. VR 203-X and VR-204-X
☐ Renewal Testing
☐ Compliance Witness
☐ Compliance Testing
☐ Engineering Evaluation
(Contractor only)
(District only)
(District only)




Facility Name:		A/C or PO Number:		Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment L)1
	CALIBRATION GAS INFORMATION2

	Calibration Gas
	Zero Gas
	Mid Range Gas
	High Range Gas

	Gas Concentration (% Propane)
	
	
	

	Serial Number
	
	
	

	Date of Last Certification
	
	
	



	Processor in manual and off mode on the TLS Console
	☐ YES
	☐ NO

	In-line ball valve upstream of the HC Sensor closed
	☐ YES
	☐ NO



	TEST RESULTS

	
Start Time3
	
Stop Time4
	Calibration Gas Percent
Concentration (% Propane)5
	Average Percent Concentration from PMC
(% Propane)6
	HC Percent Concentration Difference
(% Propane)7
	
Pass or Fail

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



	Processor returned back to automatic run mode on the TLS Console
	☐ YES
	☐ NO

	In-line ball valve upstream of the HC Sensor returned to open position
	☐ YES
	☐ NO


1 Start Time from TLS Console (The tester shall synchronize his/her watch with the clock on the TLS Console)
2 Calibration gas information listed in Section 4 of Exhibit 8 shall be attached to this form.
3 Record the start time (e.g. 09:45:00).
4 Record the stop time (e.g. 09:50:00).
5 Record the HC percent concentration of the calibration gas that was introduced into the HC sensor sample line during testing period, to the nearest hundredth (i.e. 0.01).
6 Record the average HC percent concentration from the TLS Console for the last three (3) minutes of the testing period, to the nearest hundredth (i.e. 0.01). Refer to Section 16 of the IOM for VR-203-X or Section 19 of the IOM for VR-204-X for directions on how to download the “Percent Hydrocarbon Diagnostic Report”. Attach this report to this form.
7 HC Percent Concentration Difference = Calibration Gas % Concentration – PMC % Concentration, to the nearest hundredth.
Rev 03/21	Page 1 of 1
image1.jpeg
h. San Diego County
) Air Pollution

/) Control District




