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INCON Pressure Sensor Operability Test (Balance Systems)
[bookmark: Exhibit_20_of_ARB_E.O._VR_204-X_/_Exhibi]Exhibit 20 of ARB E.O. VR 204-X / Exhibit 11 of ARB E.O. VR 208-XX


	For ISD Alarm Response Purposes Only: 1) Flow meter site glass checked to see if air is flowing:	☐ Yes	☐ No

	2) ISD Pressure sensor valve in proper orientation:	☐ Yes	☐ No



Facility Name:	A/C or PO Number:	Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing required in Attachment L).


	VAPOR PRESSURE SENSOR OFFSET CHECK (AMBIENT CHECK)

	Pressure Sensor Location:
Dispenser No.: 	/ 	
	Pressure Sensor Serial No. 	

	
	Initial Ambient Reference Check
	After calibrating the pressure sensor (If Required)10:

	Vapor Containment Area Pressure
	
	 Inches of W.C.
	
	 Inches of W.C.

	Is the sensor pressure value between
± 0.20 in w.c.?
	☐ Yes	☐ No
	☐ Yes	☐ No




	VAPOR PRESSURE SENSOR UST PRESSURE TEST

	Vapor Containment Area Pressure
			 Inches of W.C.

	UST Pressure digital manometer value
	
	 Inches of W.C.

	Is the vapor containment area pressure between ± 0.20 in w.c. of the digital manometer value?
	☐ Yes	☐ No ( (If no, the vapor pressure sensor is not in compliance. Proceed to Incon ISD system troubleshooting manual)
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