

|  |  |
| --- | --- |
| **SAN DIEGO AIR POLLUTION CONTROL DISTRICT****COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131-1649****PHONE (858) 586-2650 FAX (858) 586-2651** |  **APCD USE ONLY**  |
| SECTOR \_\_ |
| ID# \_\_\_\_\_\_ |
| NOV# \_\_\_\_\_ |

LEAK RATE OF PRESSURE/VACUUM RELIEF VENT VALVES

TP 201.1E

Facility Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ A/C or PO Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Time of Test: \_\_\_\_\_\_\_\_\_\_

(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A or L)

Grade (Check One)

[ ] 87 [ ] 89

[ ] 91 [ ] Manifold

[ ] E85

P/V Valve Manufacturer: \_\_\_\_\_\_\_\_\_\_ Model Number: \_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| Measured 2.00 inch Leak Rate (CFH): \_\_\_\_\_Positive Cracking Pressure (“w.c.): \_\_\_\_\_ Measured –4.00 inch Leak Rate (CFH): \_\_\_\_\_Negative Cracking Pressure (“w.c.): \_\_\_\_\_ |

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

Grade (Check One)

[ ] 87 [ ] 89

[ ] 91 [ ] Manifold

[ ] E85

P/V Valve Manufacturer: \_\_\_\_\_\_\_\_\_\_ Model Number: \_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| Measured 2.00 inch Leak Rate (CFH): \_\_\_\_\_Positive Cracking Pressure (“w.c.): \_\_\_\_\_ Measured –4.00 inch Leak Rate (CFH): \_\_\_\_\_Negative Cracking Pressure (“w.c.): \_\_\_\_\_ |

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

Grade (Check One)

[ ] 87 [ ] 89

[ ] 91 [ ] Manifold

[ ] E85

P/V Valve Manufacturer: \_\_\_\_\_\_\_\_\_\_ Model Number: \_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| Measured 2.00 inch Leak Rate (CFH): \_\_\_\_\_Positive Cracking Pressure (“w.c.): \_\_\_\_\_ Measured –4.00 inch Leak Rate (CFH): \_\_\_\_\_Negative Cracking Pressure (“w.c.): \_\_\_\_\_ |

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

 [ ] Pass [ ] Fail [ ] Initial Test [ ] Retest

Common conversion factors: 0.17 CFH = 80ml/min, 0.21 CFH = 100ml/min, 0.42 CFH= 200ml/min, 0.25=120ml/min

Flow Meter Calibration Date: \_\_\_\_\_\_\_\_\_\_

Pressure Manometer Calibration Date: \_\_\_\_\_\_\_\_\_\_

REV 03/21 Page 1 of 1