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COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131-1649 PHONE (858) 586-2650

[bookmark: DROP_TUBE/DRAIN_VALVE_PRESSURE_INTEGRITY]DROP TUBE/DRAIN VALVE PRESSURE INTEGRITY
[bookmark: TP_201.1C___TP_201.1D]☐ TP 201.1C	☐ TP 201.1D
Facility Name:	 A/C or PO Number:		Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A)
Drop Tube Overfill Protection Device Installed?  ☐ Yes	☐ No
UST INFORMATION: (Only required for TP 201.1D)
	Product
	Greatest Distance of SFP Measured From Bottom of Tank
	Height of Product
	Is Product > 4” above bottom of SFP?
(If no do not conduct test) Check Yes or No

	
	
	
	☐ Yes
	☐ No

	
	
	
	☐ Yes
	☐ No

	
	
	
	☐ Yes
	☐ No

	
	
	
	☐ Yes
	☐ No


TEST DATA:	Pressure measuring device calibration date: 		Flow meter calibration date: 	

	
Product Grade
	
Product Adaptor Make/ Model
	
Time (seconds) to reach
2.00 “w.c” at 0.17 CFH
	30-second stabilizing flow rate (CFH)
at 1.95” – 2.05”
	
PASS
/FAIL
	TP 201.1D only
Time (seconds) to reach 2.00 “w.c”
at 0.42 CFH
	TP 201.1D only
30-second stabilizing flow rate (CFH)
at 1.95” – 2.05”
	
QOPD=QAssembly-QDrain
	
PASS
/FAIL

	
	
	
	
	 	
	
	
	 
	
	
	
	
	 	
	
	
	 
	
	
	
	
	 	
	
	
	 
	
	
	
	
	 	
	
	
	 
	
	
	
	
	 	
	
	
	 


QOPD = The leak rate of the overfill prevention device cubic feet per hour, QASSEMBLY= The leak rate of the drop tube assembly, cubic feet per hour, QDRAIN= The leak rate of the drain valve, cubic feet per hour REV 03/21
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