[image: ] SAN DIEGO AIR POLLUTION CONTROL DISTRICT
COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131-1649 PHONE (858) 586-2650

APCD USE ONLY


SECTOR  


ID# 	


NOV# 	



LEAK RATE OF PRESSURE/VACUUM RELIEF VENT VALVES
TP 201.1E

Facility Name: 		 A/C or PO Number: 	 Time of Test: 	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A or L)


Grade (Check One)	☐87	☐ 89	☐ 91 ☐ Manifold	☐ E85

P/V Valve Manufacturer: 		Model Number: 	

REV 03/21
Page 1 of 1

Measured 2.00 inch Leak Rate (CFH): 			 Positive Cracking Pressure (“w.c.): 	 Measured –4.00 inch Leak Rate (CFH): 				 Negative Cracking Pressure (“w.c.): 		

☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest



Grade (Check One)	☐ 87	☐ 89	☐ 91 ☐ Manifold	☐ E85

P/V Valve Manufacturer: 		Model Number: 	

Measured 2.00 inch Leak Rate (CFH): 			 Positive Cracking Pressure (“w.c.): 	 Measured –4.00 inch Leak Rate (CFH): 				 Negative Cracking Pressure (“w.c.): 		

☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest



Grade (Check One)	☐ 87	☐ 89	☐ 91 ☐ Manifold	☐ E85

P/V Valve Manufacturer: 		Model Number: 	

Measured 2.00 inch Leak Rate (CFH): 			 Positive Cracking Pressure (“w.c.): 	 Measured –4.00 inch Leak Rate (CFH): 				 Negative Cracking Pressure (“w.c.): 		

☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest
☐ Pass	☐ Fail	☐ Initial Test	☐ Retest




Common conversion factors: 0.17 CFH = 80ml/min, 0.21 CFH = 100ml/min, 0.42 CFH= 200ml/min, 0.25=120ml/min

Flow Meter Calibration Date: 	

Pressure Manometer Calibration Date: 		
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