	SAN DIEGO AIR POLLUTION CONTROL DISTRICT
COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131 PHONE (858) 586-2650
	APCD USE ONLY

	
	SECTOR

	
	ID#

	
	NOV#


[bookmark: DYNAMIC_BACK_PRESSURE][image: ]DYNAMIC BACK PRESSURE
[bookmark: TP-201.4]TP-201.4

Facility Name:		A/C or PO Number:	 Time of Test:	
(Record exact time of test in order to demonstrate proper test sequencing as required in Attachment A or L)

The pressure drop shall be measured from each nozzle to the UST (methodology 1) or from the dispenser riser to the UST (methodology 4) with pressure/vacuum vent valves installed and with the poppeted Phase I vapor connection open. This test shall be performed after liquid is introduced down each dispenser riser into the Phase II system.

Test Requirements per EO VR 203-XX/204-XX/205-XX/207-XX/208-XX/209-XX Exhibit 6
	1)  Dispensers deactivated before testing?
	Yes ☐	NO ☐	NA ☐

	2)	Hirt VCS 100 Thermal Oxidizer turned off before testing? (if applicable)
	Yes ☐	NO ☐	NA ☐

	3) Nozzle and hose completely drained of gasoline prior to inserting nozzle into Dynamic Back Pressure Unit?
	Yes ☐	NO ☐	NA ☐

	4)  Nozzle lever fully engaged when conducting flow test?
	Yes ☐	NO ☐	NA ☐

	5)  Hirt VCS 100 Thermal Oxidizer turned on after testing? (If applicable)
	Yes ☐	NO ☐	NA ☐


Methodology 1	Methodology 4
	Fueling Point
	Grade Point
	Pressure Drop @
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