|  |  |
| --- | --- |
| **SAN DIEGO AIR POLLUTION CONTROL DISTRICT****COMPLIANCE DIVISION 10124 OLD GROVE ROAD SAN DIEGO CA 92131****PHONE (858) 586-2650 FAX (858) 586-2651** | **APCD USE ONLY** |
| SECTOR \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| ID#\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| NOV#\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

**Exhibit 13 of VR-203/4 and Exhibit 8 of VR-208 Hirt VCS 100 Processor Operability Test**

**Facility Name: \_ A/C or PO Number: \_\_ Date/Time of Test\*: \_**

**For ISD Alarm Response Purposes only**: Processor is on and processing vapors: **Yes** [ ]  **No**[ ]

Was TP-201.3 (Including Exhibit 4) conducted in the last 24 hours? [ ] **Yes or** [ ] **No**

Was TP-201.4 (Including Exhibit 6) conducted in the last 24 hours? [ ] **Yes or** [ ] **No**

Was Exhibit 5 conducted in the last 24 hours? [ ]  **Yes or** [ ] **No**

Was there a fuel delivery within the last 3 hours? [ ] **Yes or** [ ] **No**

Is the total ullage 70% or less of the total capacity of the GDF storage tank(s): [ ] **Yes or** [ ] **No**

|  |  |
| --- | --- |
| STEP 5.1 | Is POWER switch lit? [ ] **Yes or** [ ] **No** |
| STEP 5.2 | Is PROCESSING lamp ON? [ ] **Yes or** [ ] **No**If “YES”, test cannot be performed until lamp goes off. |
| STEP 5.9 | Time for PROCESSING Lamp to Light? \_minutesDid PROCESSING Lamp light within three (3) minutes? [ ] **Yes or** [ ] **No** |
| STEP 5.10 | Time for OVERPRESSURE Lamp to Light? \_ minutesDid OVERPRESSURE Lamp light within sixty two (62) minutes? [ ] **Yes or** [ ] **No** |